; FTDIPORT.INF
; Copyright (c) 2000-2004 FTDI Ltd.
;

[Version]
Signature="$CHICAGO$"
Class=Ports
ClassGUID={4d36e978-e325-11ce-bfc1-08002be10318}
Provider=%FTDI%
CatalogFile=ftdiport.cat
DriverVer=11/25/2004,1.09.06

[SourceDisksNames]
1=%DriversDisk%,,,

[SourceDisksFiles]
ftdiport.inf=1
;ftserui2.dll=1
;FTLang.Dll = 1

[DestinationDirs]
DefaultDestDir=11

; Install class "Ports"
;----------------------------------------------------------
[ClassInstall]
AddReg=PortsClass.AddReg

[PortsClass.AddReg]
HKR,,,,%PortsClassName%

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%FTDI%=FtdiHw

[FtdiHw]
%VID_0403&PID_8372.DeviceDesc%=FtdiPort,FTDIBUS\COMPORT&VID_0403&PID_8372
%VID_0403&PID_6001.DeviceDesc%=FtdiPort232,FTDIBUS\COMPORT&VID_0403&PID_6001
%VID_0403&PID_6007.DeviceDesc%=FtdiPort232,FTDIBUS\COMPORT&VID_0403&PID_6007
%VID_0403&PID_6008.DeviceDesc%=FtdiPort232,FTDIBUS\COMPORT&VID_0403&PID_6008
%VID_0403&PID_6009.DeviceDesc%=FtdiPort232,FTDIBUS\COMPORT&VID_0403&PID_6009
%VID_0403&PID_0232.DeviceDesc%=FtdiPort232,FTDIBUS\COMPORT&VID_0403&PID_0232

;---------------------------------------------------------------;
; For Win98 ...
;

[FtdiPort]
AddReg=FtdiPort.AddReg,FtdiPort.W98.AddReg

[FtdiPort.AddReg]
HKR,,PortSubClass,1,01

[FtdiPort.W98.AddReg]
HKR,,DevLoader,,*vcomm
HKR,,Enumerator,,ftsenum.vxd
HKR,,PortDriver,,ftcomms.vxd
HKR,,Contention,,*vcd
HKR,,ConfigDialog,,ftserui.dll
HKR,,DCB,3,1C,00,00,00, 80,25,00,00, 11,33,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,PortSubClass,1,01
HKR,,EnumPropPages,,"ftserui.dll,EnumPropPages"

[FtdiPort232]
AddReg=FtdiPort.AddReg,FtdiPort.W98.AddReg

[FtdiPort232.HW]
AddReg=FtdiPort232.HW.AddReg

[FtdiPort232.HW.AddReg]
HKR,,ConfigData,1,01,00,3F,3F,10,27,88,13,C4,09,E2,04,71,02,38,41,9c,80,4E,C0,34,00,1A,00,0D,00,06,40,03,80,00,00,d0,80


; -------------- Serenum Driver install section
[SerEnum_AddService]
DisplayName    = %SerEnum.SvcDesc%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

[FtdiPort.NT.AddReg]
HKR,,EnumPropPages32,,"ftserui2.dll,SerialPortPropPageProvider"

[FtdiPort_AddService.AddReg]
HKR,Parameters,"MaximumTransferSize",0x10001,4096
;HKR,Parameters,"DebugLevel",0x10001,2




;---------------------------------------------------------------;

[Strings]
FTDI="FTDI"
DriversDisk="FTDI USB Drivers Disk"
PortsClassName = "Ports (COM & LPT)"
VID_0403&PID_8372.DeviceDesc="USB Serial Port"
VID_0403&PID_6001.DeviceDesc="USB Serial Port"
VID_0403&PID_6007.DeviceDesc="USB Serial Port"
VID_0403&PID_6008.DeviceDesc="USB Serial Port"
VID_0403&PID_6009.DeviceDesc="USB Serial Port"
VID_0403&PID_0232.DeviceDesc="USB Serial Port"
FtdiPort.SvcDesc="USB Serial Port Driver"
SerEnum.SvcDesc="Serenum Filter Driver"


